{"text_format":"3","workbook":"xlsx","n_sheets":5,"sheets":["一级场镇有排污许可证监测指标及频次","一级场镇无排污许可证监测指标及频次","二级场镇监测指标及频次","农村示范点监测指标及频次","监测总次数及价格统计"],"read":"whole","date_system":"1900"}

{"sheet":"一级场镇有排污许可证监测指标及频次","index":0,"n_rows":28,"n_cols":8,"rows_kept":28,"merged":[[0,0,0,7],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[8,0,9,0],[8,1,9,1],[8,2,9,2],[8,3,9,3],[10,0,11,0],[10,1,11,1],[10,2,11,2],[10,3,11,3],[12,0,13,0],[12,1,13,1],[12,2,13,2],[12,3,13,3],[14,0,15,0],[14,1,15,1],[14,2,15,2],[14,3,15,3],[16,0,17,0],[16,1,17,1],[16,2,17,2],[16,3,17,3],[18,0,19,0],[18,1,19,1],[18,2,19,2],[18,3,19,3],[20,0,21,0],[20,1,21,1],[20,2,21,2],[20,3,21,3],[22,0,23,0],[22,1,23,1],[22,2,23,2],[22,3,23,3],[24,0,25,0],[24,1,25,1],[24,2,25,2],[24,3,25,3],[26,0,27,0],[26,1,27,1],[26,2,27,2],[26,3,27,3]]}
["泸州市汇鑫环保科技有限公司\n污水处理中心一级场镇有排污许可证第三方检测指标、频次统计表\n《城镇污水处理厂污染物排放标准》GB18918-2002一级A标准"]
["序号","项目编号","项目名称","项目地址","监测点位","季度检测指标","半年监测指标","年度监测指标"]
[1,2023033001,"尧坝镇生活污水处理厂","泸州市合江县尧坝镇","进口","pH值、化学需氧量、氨氮、总氮、总磷","无","无"]
[{"$nulls":4},"出口","色度、五日生化需氧量、石油类、动植物油类、阴离子表面活性剂、pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷","总汞、总铬、六价铬、总砷、总镉、烷基汞、\n臭气浓度、氨（氨气）、硫化氢、噪声、污泥含水率","甲烷"]
[2,2023033002,"先市镇生活污水处理厂","泸州市合江县先市镇","进口","pH值、化学需氧量、氨氮、总氮、总磷","无","无"]
[{"$nulls":4},"出口","色度、五日生化需氧量、石油类、动植物油类、阴离子表面活性剂、pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷","总汞、总铬、六价铬、总砷、总镉、烷基汞、\n臭气浓度、氨（氨气）、硫化氢、噪声、污泥含水率","甲烷"]
[3,2023033003,"凤鸣镇生活污水处理厂","泸州市合江县凤鸣镇","进口","pH值、化学需氧量、氨氮、总氮、总磷","无","无"]
[{"$nulls":4},"出口","色度、五日生化需氧量、石油类、动植物油类、阴离子表面活性剂、pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷","总汞、总铬、六价铬、总砷、总镉、烷基汞、\n臭气浓度、氨（氨气）、硫化氢、噪声","甲烷"]
[4,2023033004,"先滩镇先滩生活污水处理厂","泸州市合江县先滩镇","进口","pH值、化学需氧量、氨氮、总氮、总磷","无","无"]
[{"$nulls":4},"出口","色度、五日生化需氧量、石油类、动植物油类、阴离子表面活性剂、pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷","总汞、总铬、六价铬、总砷、总镉、烷基汞、\n臭气浓度、氨（氨气）、硫化氢、噪声","甲烷"]
[5,2023033005,"白鹿镇生活污水处理厂","泸州市合江县白鹿镇","进口","pH值、化学需氧量、氨氮、总氮、总磷","无","无"]
[{"$nulls":4},"出口","色度、五日生化需氧量、石油类、动植物油类、阴离子表面活性剂、pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷","总汞、总铬、六价铬、总砷、总镉、烷基汞、\n臭气浓度、氨（氨气）、硫化氢、噪声","甲烷"]
[6,2023033006,"白米镇生活污水处理厂","泸州市合江县白米镇","进口","pH值、化学需氧量、氨氮、总氮、总磷","无","无"]
[{"$nulls":4},"出口","色度、五日生化需氧量、石油类、动植物油类、阴离子表面活性剂、pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷","总汞、总铬、六价铬、总砷、总镉、烷基汞、\n臭气浓度、氨（氨气）、硫化氢、噪声、污泥含水率","甲烷"]
[7,2023033007,"大桥镇佛荫生活污水处理厂","泸州市合江县大桥镇","进口","pH值、化学需氧量、氨氮、总氮、总磷","无","无"]
[{"$nulls":4},"出口","色度、五日生化需氧量、石油类、动植物油类、阴离子表面活性剂、pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷","总汞、总铬、六价铬、总砷、总镉、烷基汞、\n臭气浓度、氨（氨气）、硫化氢、噪声、污泥含水率","甲烷"]
[8,2023033008,"甘雨镇生活污水处理厂","泸州市合江县甘雨镇","进口","pH值、化学需氧量、氨氮、总氮、总磷","无","无"]
[{"$nulls":4},"出口","色度、五日生化需氧量、石油类、动植物油类、阴离子表面活性剂、pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷","总汞、总铬、六价铬、总砷、总镉、烷基汞、\n臭气浓度、氨（氨气）、硫化氢、噪声","甲烷"]
[9,2023033009,"临港街道污水处理厂","泸州市合江县\n临港街道","进口","pH值、化学需氧量、氨氮、总氮、总磷","无","无"]
[{"$nulls":4},"出口","总汞、总铬、六价铬、总砷、总镉、烷基汞、色度、五日生化需氧量、石油类、动植物油类、阴离子表面活性剂、pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷","臭气浓度、氨（氨气）、硫化氢、噪声、污泥含水率","甲烷"]
[10,2023033010,"福宝污水处理厂","泸州市合江县福宝镇","进口","pH值、化学需氧量、氨氮、总氮、总磷","无","无"]
[{"$nulls":4},"出口","色度、五日生化需氧量、石油类、动植物油类、阴离子表面活性剂、pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷","总汞、总铬、六价铬、总砷、总镉、烷基汞、\n臭气浓度、氨（氨气）、硫化氢、噪声、污泥含水率","甲烷"]
[11,2023033011,"白沙镇污水处理厂","泸州市合江县白沙镇","进口","pH值、化学需氧量、氨氮、总氮、总磷","无","无"]
[{"$nulls":4},"出口","色度、五日生化需氧量、石油类、动植物油类、阴离子表面活性剂、pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷","总汞、总铬、六价铬、总砷、总镉、烷基汞、\n臭气浓度、氨（氨气）、硫化氢、噪声、污泥含水率","甲烷"]
[12,2023033012,"神臂城污水处理厂","泸州市合江县\n神臂城镇","进口","pH值、化学需氧量、氨氮、总氮、总磷","无","无"]
[{"$nulls":4},"出口","色度、五日生化需氧量、石油类、动植物油类、阴离子表面活性剂、pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷","总汞、总铬、六价铬、总砷、总镉、烷基汞、\n臭气浓度、氨（氨气）、硫化氢、噪声、污泥含水率","甲烷"]
[13,2023033013,"荔江镇堰坝污水处理厂","泸州市合江县\n荔江镇堰坝","进口","pH值、化学需氧量、氨氮、总氮、总磷","无","无"]
[{"$nulls":4},"出口","色度、五日生化需氧量、石油类、动植物油类、阴离子表面活性剂、pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷","总汞、总铬、六价铬、总砷、总镉、烷基汞、\n臭气浓度、氨（氨气）、硫化氢、噪声、污泥含水率","甲烷"]

{"sheet":"一级场镇无排污许可证监测指标及频次","index":1,"n_rows":20,"n_cols":7,"rows_kept":20,"merged":[[0,0,0,6],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,6,19,6],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[8,0,9,0],[8,1,9,1],[8,2,9,2],[8,3,9,3],[10,0,11,0],[10,1,11,1],[10,2,11,2],[10,3,11,3],[12,0,13,0],[12,1,13,1],[12,2,13,2],[12,3,13,3],[14,0,15,0],[14,1,15,1],[14,2,15,2],[14,3,15,3],[16,0,17,0],[16,1,17,1],[16,2,17,2],[16,3,17,3],[18,0,19,0],[18,1,19,1],[18,2,19,2],[18,3,19,3]]}
["泸州市汇鑫环保科技有限公司\n污水处理中心一级场镇无排污许可证第三方检测指标、频次统计表\n《城镇污水处理厂污染物排放标准》GB18918-2002一级A标准"]
["序号","项目编号","项目名称","项目地址","监测点位","监测指标","监测频次"]
[1,2023033014,"望龙镇生活污水处理厂","泸州市合江县望龙镇","进口","pH值、化学需氧量、氨氮、总氮、总磷","每季度一次"]
[{"$nulls":4},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[2,2023033015,"真龙镇生活污水处理厂","泸州市合江县真龙镇","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":4},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[3,2023033016,"白米镇生活污水处理厂\n（转龙湾）","泸州市合江县白米镇","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":4},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[4,2023033017,"石龙镇南滩生活污水处理厂","泸州市合江县石龙镇","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":4},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[5,2023033018,"法王寺镇生活污水处理厂（1）","泸州市合江县法王寺镇","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":4},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[6,2023033019,"法王寺镇生活污水处理厂（2）","泸州市合江县法王寺镇","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":4},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[7,2023033020,"车辋镇生活污水处理厂","泸州市合江县车辋镇","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":4},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[8,2023033021,"榕山镇榕右生活污水处理厂","泸州市合江县榕山镇","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":4},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[9,2023033022,"荔江镇生活污水处理厂","泸州市合江县荔江镇","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":4},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]

{"sheet":"二级场镇监测指标及频次","index":2,"n_rows":34,"n_cols":8,"rows_kept":34,"merged":[[0,0,0,7],[2,0,3,0],[2,1,3,1],[2,2,25,2],[2,3,3,3],[2,4,3,4],[2,7,33,7],[4,0,5,0],[4,1,5,1],[4,3,5,3],[4,4,5,4],[6,0,7,0],[6,1,7,1],[6,3,7,3],[6,4,7,4],[8,0,9,0],[8,1,9,1],[8,3,9,3],[8,4,9,4],[10,0,11,0],[10,1,11,1],[10,3,11,3],[10,4,11,4],[12,0,13,0],[12,1,13,1],[12,3,13,3],[12,4,13,4],[14,0,15,0],[14,1,15,1],[14,3,15,3],[14,4,15,4],[16,0,17,0],[16,1,17,1],[16,3,17,3],[16,4,17,4],[18,0,19,0],[18,1,19,1],[18,3,19,3],[18,4,19,4],[20,0,21,0],[20,1,21,1],[20,3,21,3],[20,4,21,4],[22,0,23,0],[22,1,23,1],[22,3,23,3],[22,4,23,4],[24,0,25,0],[24,1,25,1],[24,3,25,3],[24,4,25,4],[26,0,27,0],[26,1,27,1],[26,2,33,2],[26,3,27,3],[26,4,27,4],[28,0,29,0],[28,1,29,1],[28,3,29,3],[28,4,29,4],[30,0,31,0],[30,1,31,1],[30,3,31,3],[30,4,31,4],[32,0,33,0],[32,1,33,1],[32,3,33,3],[32,4,33,4]]}
["泸州市汇鑫环保科技有限公司\n污水处理中心二级场镇第三方检测指标、频次统计表"]
["序号","编号","标准","厂区","地址","采样点","监测指标","监测频次"]
[1,2023033023,"\n《省农村一级标准》db51/2626-2019\n","先滩镇自怀生活污水处理厂","泸州市合江县先滩镇","进口","pH值、化学需氧量、氨氮、总氮、总磷","每季度一次"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[2,2023033024,null,"石龙镇石龙生活污水处理厂","泸州市合江县石龙镇","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[3,2023033025,null,"荔江镇实录生活污水处理厂","泸州市合江县荔江镇","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[4,2023033026,null,"车辋镇桂花场污水处理站","泸州市合江县车辋镇桂花场","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[5,2023033027,null,"先市镇新店场污水处理站","泸州市合江县先市镇新店场","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[6,2023033028,null,"白沙镇忘川场污水处理站","泸州市合江县白沙镇忘川场","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[7,2023033029,null,"尧坝镇识字场污水处理站","泸州市合江县尧坝镇识字场","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[8,2023033030,null,"神臂城镇临江场污水处理站","泸州市合江县神臂城镇临江场","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[9,2023033031,null,"法王寺镇石佛场污水处理站","泸州市合江县法王寺镇石佛场","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[10,2023033032,null,"甘雨镇油榨场污水处理站","泸州市合江县甘雨镇油榨场","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[11,2023033033,null,"榕右乡永安场污水处理站","泸州市合江县榕右乡永安场","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[12,2023033034,null,"先滩镇民建场污水处理站","泸州市合江县先滩镇民建场","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[13,2023033035,"《城镇污水处理厂污染物排放标准》\nGB18918-2002一级A标准\n","白沙镇参宝污水处理厂","泸州市合江县白沙镇凉石坪","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[14,2023033036,null,"九支镇五通污水处理厂","泸州市合江县九支镇五通","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[15,2023033037,null,"荔江镇河坝污水处理厂","泸州市合江县荔江镇河坝","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[16,2023033038,null,"大桥镇大桥生活污水处理厂","泸州市合江县大桥镇","进口","pH值、化学需氧量、氨氮、总氮、总磷"]
[{"$nulls":5},"出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]

{"sheet":"农村示范点监测指标及频次","index":3,"n_rows":37,"n_cols":6,"rows_kept":37,"merged":[[0,0,0,5],[1,0,1,5],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[6,0,7,0],[6,1,7,1],[6,2,7,2],[6,3,7,3],[6,4,7,4],[6,5,7,5],[8,0,9,0],[8,1,9,1],[8,2,9,2],[8,3,9,3],[8,4,9,4],[8,5,9,5],[10,0,11,0],[10,1,11,1],[10,2,11,2],[10,3,11,3],[10,4,11,4],[10,5,11,5],[12,0,13,0],[12,1,13,1],[12,2,13,2],[12,3,13,3],[12,4,13,4],[12,5,13,5],[14,0,15,0],[14,1,15,1],[14,2,15,2],[14,3,15,3],[14,4,15,4],[14,5,15,5],[16,0,17,0],[16,1,17,1],[16,2,17,2],[16,3,17,3],[16,4,17,4],[16,5,17,5],[18,0,19,0],[18,1,19,1],[18,2,19,2],[18,3,19,3],[18,4,19,4],[18,5,19,5],[20,0,21,0],[20,1,21,1],[20,2,21,2],[20,3,21,3],[20,4,21,4],[20,5,21,5],[22,0,23,0],[22,1,23,1],[22,2,23,2],[22,3,23,3],[22,4,23,4],[22,5,23,5],[24,0,25,0],[24,1,25,1],[24,2,25,2],[24,3,25,3],[24,4,25,4],[24,5,25,5],[26,0,27,0],[26,1,27,1],[26,2,27,2],[26,3,27,3],[26,4,27,4],[26,5,27,5],[28,0,29,0],[28,1,29,1],[28,2,29,2],[28,3,29,3],[28,4,29,4],[28,5,29,5],[30,0,31,0],[30,1,31,1],[30,2,31,2],[30,3,31,3],[30,4,31,4],[30,5,31,5],[32,0,33,0],[32,1,33,1],[32,2,33,2],[32,3,33,3],[32,4,33,4],[32,5,33,5],[34,0,35,0],[34,1,35,1],[34,2,35,2],[34,3,35,3],[34,4,35,4],[34,5,35,5],[36,0,36,5]]}
["泸州汇鑫环保科技有限公司污水处理中心\n农村示范点第三方检测指标统计表"]
["《省农村一级标准》db51/2626-2019 排放限值：COD：60； TN：20；NH3-N：8（15）；TP:1.5；一年监测两次"]
[1,2023033039,"望龙镇永定村污水处理站","泸州市合江县望龙镇永定村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[2,2023033040,"白米镇梨湾村污水处理站","泸州市合江县白米镇梨湾村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[3,2023033041,"参宝镇会龙村污水处理站","泸州市合江县参宝镇会龙村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[4,2023033042,"参宝镇龙顶山村污水处理站","泸州市合江县参宝镇龙顶山村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[5,2023033043,"神臂城镇高陵村污水处理站","泸州市合江县神臂城镇高陵村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[6,2023033044,"佛荫镇流石村污水处理站","泸州市合江县佛荫镇流石村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[7,2023033045,"白鹿镇水竹村污水处理站","泸州市合江县白鹿镇水竹村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[8,2023033046,"佛荫镇乘山村污水处理站","泸州市合江县佛荫镇乘山村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[9,2023033047,"大桥镇望龙山村污水处理站","泸州市合江县大桥镇望龙山村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[10,2023033048,"自怀镇天池村污水处理站","泸州市合江县自怀镇天池村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[11,2023033049,"大桥镇长江村污水处理站","泸州市合江县大桥镇长江村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[12,2023033050,"榕山镇小羊洞村污水处理站","泸州市合江县榕山镇小羊洞村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[13,2023033051,"榕山镇回洞桥村污水处理站","泸州市合江县榕山镇回洞桥村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[14,2023033052,"甘雨镇槐花村污水处理站","泸州市合江县甘雨镇槐花村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[15,2023033053,"甘雨镇黄桷村污水处理站","泸州市合江县甘雨镇黄桷村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[16,2023033054,"望龙镇鹿角场污水处理站","泸州市合江县望龙镇鹿角场","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
[17,2023033055,"白沙镇风岩村污水处理站","泸州市合江县白沙镇风岩村","出口","pH值、粪大肠菌群、悬浮物、化学需氧量、氨氮、总氮、总磷"]
[]
["备注：九支月台、五通李嘴、合江魏家祠、石龙太平几个厂区无进水，暂不监测。"]

{"sheet":"监测总次数及价格统计","index":4,"n_rows":27,"n_cols":8,"rows_kept":27,"merged":[[0,0,0,7],[2,0,13,0],[2,1,13,1],[2,2,13,2],[2,7,13,7],[14,0,20,0],[14,1,20,1],[14,2,20,2],[14,7,20,7],[21,0,24,0],[21,1,24,1],[21,2,24,2],[21,7,24,7],[27,0,27,7]]}
["泸州汇鑫环保科技有限公司\n污水处理中心第三方水质检测项目总频次统计表"]
["序号","检测项目","监测厂区","指标","年检测频次","单价（元）","共计（元）","备注"]
[1,"排水口常规项 \n（12 项）",null,"化学需氧量",338,null,null,"每次检测采集瞬时水样\n至少三个瞬时样"]
[{"$nulls":3},"氨氮",338]
[{"$nulls":3},"总磷",338]
[{"$nulls":3},"总氮",338]
[{"$nulls":3},"pH值",338]
[{"$nulls":3},"五日生化需氧量",52]
[{"$nulls":3},"悬浮物",186]
[{"$nulls":3},"色度",52]
[{"$nulls":3},"动植物油",52]
[{"$nulls":3},"粪大肠菌群",186]
[{"$nulls":3},"石油类",52]
[{"$nulls":3},"阴离子表面活性剂",52]
[2,"排水口重金属 离子\n（7项）",null,"总汞",28,null,null,"每次检测采集瞬时水样\n至少三个瞬时样"]
[{"$nulls":3},"总镉",28]
[{"$nulls":3},"总铭",28]
[{"$nulls":3},"总铅",28]
[{"$nulls":3},"总砷",28]
[{"$nulls":3},"六价铭",28]
[{"$nulls":3},"烷基汞",28]
[3,"废气\n（4项）",null,"氨",26,null,null,"每次检测要求非连续采样\n至少三次"]
[{"$nulls":3},"臭气",26]
[{"$nulls":3},"硫化氢",26]
[{"$nulls":3},"甲烷",13]
[4,"噪声",null,"厂界环境噪声",26,null,null,"昼间、夜间分别测定"]
[5,"污泥",null,"污泥含水率",18,null,null,"每次检测采集三个点位样品"]